Packet Tracer PC Command Line 1.0

C:\>ipconfig /all

FastEthernet0 Connection:(default port)

Connection-specific DNS Suffix..:

Physical Address................: 0060.47CA.4DEE

Link-local IPv6 Address.........: FE80::260:47FF:FECA:4DEE

IPv6 Address....................: ::

IPv4 Address....................: 10.10.1.98

Subnet Mask.....................: 255.255.255.224

Default Gateway.................: ::

10.10.1.97

DHCP Servers....................: 0.0.0.0

DHCPv6 IAID.....................:

DHCPv6 Client DUID..............: 00-01-00-01-B2-33-AD-8B-00-60-47-CA-4D-EE

DNS Servers.....................: ::

0.0.0.0

Bluetooth Connection:

Connection-specific DNS Suffix..:

Physical Address................: 000C.8599.E691

Link-local IPv6 Address.........: ::

C:\>ping 10.10.1.18

Pinging 10.10.1.18 with 32 bytes of data:

Reply from 10.10.1.97: Destination host unreachable.

Reply from 10.10.1.97: Destination host unreachable.

Reply from 10.10.1.97: Destination host unreachable.

Reply from 10.10.1.97: Destination host unreachable.

Ping statistics for 10.10.1.18:

Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

C:\>tracert 10.10.1.18

Tracing route to 10.10.1.18 over a maximum of 30 hops:

1 1 ms 0 ms 0 ms 10.10.1.97

2 0 ms \* 1 ms 10.10.1.97

3 \* 3 ms \* Request timed out.

4 0 ms \* 3 ms 10.10.1.97

5 \* 0 ms \* Request timed out.

6 4 ms \* 0 ms 10.10.1.97

7

Control-C

^C

C:\>ping 10.10.1.18

Pinging 10.10.1.18 with 32 bytes of data:

Reply from 10.10.1.18: bytes=32 time=3ms TTL=125

Reply from 10.10.1.18: bytes=32 time=10ms TTL=125

Reply from 10.10.1.18: bytes=32 time=18ms TTL=125

Reply from 10.10.1.18: bytes=32 time=2ms TTL=125

Ping statistics for 10.10.1.18:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),

Approximate round trip times in milli-seconds:

Minimum = 2ms, Maximum = 18ms, Average = 8ms