User Access Verification

Password:

R2>en

Password:

R2#show ip interface brief

Interface IP-Address OK? Method Status Protocol

GigabitEthernet0/0 unassigned YES unset administratively down down

GigabitEthernet0/1 unassigned YES unset administratively down down

Serial0/0/0 10.10.1.2 YES manual up up

Serial0/0/1 10.10.1.9 YES manual up up

Vlan1 unassigned YES unset administratively down down

R2#conf t

Enter configuration commands, one per line. End with CNTL/Z.

R2(config)#interface s0/0/0

R2(config-if)#ip address 10.10.1.5 255.255.255.252

R2(config-if)#

%DUAL-5-NBRCHANGE: IP-EIGRP 1: Neighbor 10.10.1.6 (Serial0/0/0) is up: new adjacency

R2(config-if)#no shutdown