R1>en

R1#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.

R1(config)#interface G0/0

R1(config-if)#ip helper-address 10.1.1.2

R1#ping 192.168.10.0

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.10.0, timeout is 2 seconds:

Reply to request 0 from 192.168.10.11, 1 ms

Reply to request 1 from 192.168.10.11, 1 ms

Reply to request 2 from 192.168.10.11, 0 ms

Reply to request 3 from 192.168.10.11, 0 ms

Reply to request 4 from 192.168.10.11, 0 ms