R3>en

R3#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.

R3(config)#interface G0/0

R3(config-if)#ip helper-address 10.2.2.2

R3>ping 192.168.10.0

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.10.0, timeout is 2 seconds:

!!!!!

Success rate is 100 percent (5/5), round-trip min/avg/max = 2/9/13 ms