C:\>ipconfig

FastEthernet0 Connection:(default port)

Connection-specific DNS Suffix..:

Link-local IPv6 Address.........: FE80::2

IPv6 Address....................: 2001:DB8:ACAD:1::2

IPv4 Address....................: 172.16.2.3

Subnet Mask.....................: 255.255.255.0

Default Gateway.................: FE80::1

172.16.2.1

Bluetooth Connection:

Connection-specific DNS Suffix..:

Link-local IPv6 Address.........: ::

IPv6 Address....................: ::

IPv4 Address....................: 0.0.0.0

Subnet Mask.....................: 0.0.0.0

Default Gateway.................: ::

0.0.0.0

C:\>ping 209.165.201.2

Pinging 209.165.201.2 with 32 bytes of data:

Request timed out.

Request timed out.

Request timed out.

Request timed out.

Ping statistics for 209.165.201.2:

Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

C:\>ping 172.16.2.1

Pinging 172.16.2.1 with 32 bytes of data:

Request timed out.

Request timed out.

Request timed out.

Request timed out.

Ping statistics for 172.16.2.1:

Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

C:\>ping 172.16.2.4

Pinging 172.16.2.4 with 32 bytes of data:

Reply from 172.16.2.4: bytes=32 time=1ms TTL=128

Reply from 172.16.2.4: bytes=32 time<1ms TTL=128

Reply from 172.16.2.4: bytes=32 time=1ms TTL=128

Reply from 172.16.2.4: bytes=32 time<1ms TTL=128

Ping statistics for 172.16.2.4:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),

Approximate round trip times in milli-seconds:

Minimum = 0ms, Maximum = 1ms, Average = 0ms

C:\>ping 172.16.1.3

Pinging 172.16.1.3 with 32 bytes of data:

Request timed out.

Request timed out.

Request timed out.

Request timed out.

Ping statistics for 172.16.1.3:

Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

C:\>ping 172.16.1.4

Pinging 172.16.1.4 with 32 bytes of data:

Request timed out.

Request timed out.

Request timed out.

Request timed out.

Ping statistics for 172.16.1.4:

Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),